**Apalachicola (APA) NERR Meteorological Metadata**

**January 2021 – December 2021**

**Latest Update: August 10, 2022**

**I. Data Set and Research Descriptors**

**1) Principal investigator(s) and contact persons –**

Jason Garwood, Research Coordinator

[Jason.garwood@dep.state.fl.us](mailto:Jason.garwood@dep.state.fl.us)

850-670-7705

Ethan Bourque, Environmental Specialist

[Ethan.bourque@dep.state.fl.us](mailto:Ethan.bourque@dep.state.fl.us)

850-670-7722

Florida Department of Environmental Protection

Apalachicola National Estuarine Research Reserve

108 Island Drive

Eastpoint, FL 32328

**2) Entry verification –**

Data are uploaded from the CR1000X data logger to a Personal Computer (IBM compatible). Files are exported from LoggerNet in a comma-delimited format and uploaded to the CDMO where they undergo automated primary QAQC and become part of the CDMO’s online provisional database. During primary QAQC, data are flagged if they are missing or out of sensor range. The edited file is then returned to the Reserve where it is opened in Microsoft Excel and processed using the CDMO’s NERRQAQC Excel macro. The macro inserts station codes, creates metadata worksheets for flagged data and summary statistics, and graphs the data for review. It allows the user to apply QAQC flags and codes to the data, append files, and export the resulting data file to the CDMO for tertiary QAQC and assimilation into the CDMO’s authoritative online database. For more information on QAQC flags and QAQC codes, see Sections 11 and 12.

Ethan Bourque is responsible for all Meteorological data management with assistance from Jason Garwood.

**3) Research objectives –**

The objective of this research is to monitor meteorological data on a long-term basis. Data collected from the East Bay weather station complement those data taken from the East Bay water quality station. Data are also used in the analysis of other datalogger data collected at Cat Point, Dry Bar, Pilots Cove, and Little St. Marks. Weather station data will also be integrated with monitoring the Reserve is performing as a Sentinel Site for climate change. Positioning the weather station in East Bay allows the Reserve to monitor changes in rainfall, photosynthetically active radiation, temperature, and other weather parameters influencing the water quality of East Bay as well as climate change sentinel sites located in East Bay marshes. East Bay drains the Tate's Hell Swamp area, which was altered in the late 1960's and early 1970's by timber companies. An EPA grant allowed the Northwest Florida Water Management District to begin restoration of the site in 1995 to reduce non-point source runoff. East Bay is also an important nursery area for numerous fish and invertebrate species within Apalachicola Bay.

**4) Research methods –**

Campbell Scientific data telemetry equipment was installed at the East Bay weather station on 06/22/2006 and transmits data to the NOAA GOES satellite, NESDIS ID #3B01C09E. The transmissions are scheduled hourly at 0:00:50 and contain four (4) data sets reflecting fifteen-minute data sampling intervals. Upon receipt by the CDMO, the data undergoes the same automated primary QAQC process detailed in Section 2 above. The “real-time” telemetry data become part of the provisional dataset until undergoing secondary and tertiary QAQC and assimilation in the CDMO’s authoritative online database. Provisional and authoritative data are available at http://cdmo.baruch.sc.edu.

Data are collected in Eastern Standard Time (EST) for the entire year.

Data Collection (CR1000X):

The 15-minute data are collected in the following formats for the CR1000X:

Averages from 5-second data:

Air Temperature (°C), Relative Humidity (%), Barometric Pressure (mb), Wind Speed (m/s), Wind Direction (degrees), Battery Voltage (volts)

Maximum and Minimum Air Temperature (°C) and their times from 5-second data (these data are available from the reserve)

Maximum Wind Speed (m/s) and time from 5-second data

Wind Direction Standard Deviation (degrees)

Totals:

Precipitation (mm), PAR (millimoles/m2), and Cumulative Precipitation (mm) (Cumulative precipitation is no longer available via export from the CDMO. Please contact the reserve or the CDMO for more information or to obtain these data.)

Sensor Calibration QA/QC:

Sensors are calibrated either yearly or every 2 years according to the maintenance schedule dictated by the NERR System Wide Monitoring Program SOPs. The sensors and their wires are inspected monthly to make sure that they are clean, moving freely, and undamaged. The arm of the wind sensor is checked monthly to assure that it is aligned to true north.

Recommended calibration frequency for the MET station sensors:

- Temperature/Humidity- yearly recalibration

- Rain Gauge- yearly recalibration

- Wind Speed/Direction- every 2 years recalibration for the RM Young 5103 sensor

- Barometric Pressure- every 2 years recalibration

- PAR- every 2 years recalibration

- CR1000X- every 5 years (required beginning 2014)

Data Storage/Interface with LoggerNet:

A Laptop is used to interface between the CR1000X and the LoggerNet software supplied by Campbell Scientific. Data is downloaded monthly and at the time of the download, a handheld Kestrel 4000 is used to measure weather conditions and compare them to the measurements of the sensors on the weather station. A neighboring weather station operated by Florida Department of Environmental Protection, Division of State Lands, is used for further comparison when necessary.

**5) Site location and character –**

The Apalachicola National Estuarine Research Reserve is located in the northwestern part of Florida, generally called the panhandle. It is located adjacent to the City of Apalachicola, and encompasses most of the Apalachicola Bay system, including 52 miles of the lower Apalachicola River. Passes, both natural and manmade, connect Apalachicola Bay to the northeastern Gulf of Mexico. The sampling site is located in the upper reaches of East Bay. East Bay is separated from Apalachicola Bay by two bridges and a causeway and is located to the north of Apalachicola Bay proper. The bay is 8.2 km long, has an average depth of approximately 1.0 m MHW, and an average width of 1.8 km. The tides in East Bay are mixed and range from 0.3 m to 1.0 m (average 0.5 m).

The weather station was located at latitude 29 47' 27.24 N and longitude 84 53' 0.24 W but was moved to latitude 29°46'9.78" N and longitude 84°52'53.35" W following serious damage from Hurricane Michael in 2018. This new site is roughly 2 nautical miles south southeast of the original location and roughly 1.8 nautical miles south southwest of the East Bay water quality station. The site is located in upper East Bay at the end of the dock at the Carrol Street office. The area is dominated by marsh vegetation (mainly Juncus roemerianus). The dominant upland habitat is primarily pineland forest, which includes slash pine, saw palmetto, and sand pine. In accordance with NERR SWMP and CDMO requirements the weather station wind and PAR sensors are mounted at the top of a 3-meter tower. The temperature/relative humidity sensor and barometric pressure sensor (inside the CR1000 enclosure) are mounted on the tower at 1.5 meters. The tower is mounted on an approximately 3 meter tall dock. The tipping bucket rain gauge is mounted on a 1.2 meter platform approximately 3.5 meters from the weather station tower. There is nothing nearby to shade the tower and the nearest wind block is the edge of the small pine forest about 0.1 kilometer southeast of the station.

SWMP Station Timeline:

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Station Code | SWMP Status | Station Name | Location | Active Dates | Reason Decommissioned | Notes |
| APAEBMET | P | East Bay | 29°47'27.24"N 84°53'0.24"W | 01/01/2001 – 12/31/2018 | Station damaged by hurricane Michael | Structure began to sink |
| APAEBMET | P | East Bay | 29°46'9.78"N 84°52'53.35"W | 09/03/2019 - current | NA | NA |

**6) Data collection period –**

The Apalachicola weather monitoring station was erected on August 27, 1999 and began monitoring on September 3, 1999. The data submitted with this report encompasses data collected from 00:00 January 1, 2021 through 23:45 December 31, 2021.

|  |  |  |
| --- | --- | --- |
| **Raw File Name** | **Start Date/Time** | **End Date/Time** |
| Apaebmet120820 | 12/08/2020 10:15 | 01/14/2021 009:30 |
| Apaebmet011421 | 01/14/2021 09:45 | 02/04/2021 11:15 |
| Apaebmet020421 | 02/04/2021 11:30 | 03/05/2021 10:00 |
| Apaebmet030521 | 03/02/2021 10:15 | 04/01/2021 10:45 |
| Apaebmet040121 | 04/01/2021 11:00 | 05/10/2021 07:30 |
| Apaebmet051021 | 05/10/2021 07:45 | 06/04/2021 12:00 |
| Apaebmet060421 | 06/04/2021 12:15 | 07/02/2021 13:15 |
| Apaebmet070221 | 07/02/2021 13:30 | 08/05/2021 09:45 |
| Apaebmet080521 | 08/05/2021 10:00 | 09/02/2021 09:15 |
| Apaebmet090221 | 09/02/2021 09:30 | 09/30/2021 09:30 |
| Apaebmet100721 | 10/07/2021 09:45 | 10/23/2021 17:30 |
| Apaebmet102521 | 10/25/2021 13:45 | 11/08/2021 10:15 |
| Apaebmet110821 | 11/08/2021 10:30 | 12/06/2021 10:00 |
| Apaebmet120621 | 12/06/2021 10:15 | 01/06/2022 12:30 |

**7) Distribution –**

NOAA retains the right to analyze, synthesize and publish summaries of the NERRS System-wide Monitoring Program data.  The NERRS retains the right to be fully credited for having collected and processed the data.  Following academic courtesy standards, the NERR site where the data were collected should be contacted and fully acknowledged in any subsequent publications in which any part of the data are used.  The data set enclosed within this package/transmission is only as good as the quality assurance and quality control procedures outlined by the enclosed metadata reporting statement.  The user bears all responsibility for its subsequent use/misuse in any further analyses or comparisons.  The Federal government does not assume liability to the Recipient or third persons, nor will the Federal government reimburse or indemnify the Recipient for its liability due to any losses resulting in any way from the use of this data.

Requested citation format:

NOAA National Estuarine Research Reserve System (NERRS). System-wide Monitoring Program. Data accessed from the NOAA NERRS Centralized Data Management Office website: <http://www.nerrsdata.org/>; *accessed* 12 October 2021.

NERR meteorological data and metadata can be obtained from the Research Coordinator at the individual NERR site (please see Principal Investigators and Contact Persons), from the Data Manager at the Centralized Data Management Office (please see personnel directory under the general information link on the CDMO home page) and online at the CDMO home page [www.nerrsdata.org](http://www.nerrsdata.org).  Data are available in comma delimited format.

**8) Associated researchers and projects –**

Harper, J., Wren, K., Jones, D., Garwood, J., Garland, H., Snyder, C., Levi, L., Bourque, E./ NERRS Sentinel Sites Program for Understanding Climate Change Impacts on Estuaries

Edmiston, H.L., Farhny, S., Lamb, M., Levi, L., Wanat, J., Avant, J., Selly, N. Apalachicola National Estuarine Research Reserve. Tropical Storm and Hurricane Impacts on a Gulf Coast Estuary: Apalachicola Bay, Florida USA.

Garwood, J., Harper, J., Levi, L., Lamb, M., Jones, D., Garland, H., Bourque, E., Yuan, W., Christopher, M., Cox, N. Apalachicola National Estuarine Research Reserve. Distribution and density of fishes and benthic invertebrates in Apalachicola Bay.

Harper, J., Levi, L., Jones, D., Lamb, M., Garwood, J., Garland, H., Bourque, E. Apalachicola National Estuarine Research Reserve. System-Wide Monitoring Program (SWMP) for water quality, weather, nutrients & chlorophyll A, and submerged aquatic vegetation monitoring in Apalachicola Bay.

Gilhring, T. Florida State University. The role of oligohaline marshes as a source or sink of nitrogen to the Apalachicola Bay.

Peterson, R. Florida State University. Origin and fate of suspended particulates in the Apalachicola River: Impact on Apalachicola Bay.

Putland, J. Florida State University Department of Oceanography. NOAA Graduate Research Fellowship. Planktonic food web variations related to salinity and nutrient patterns in Apalachicola Bay.

Wang, H., Huang, W., Harwell, M., Edmiston, H.L., Johnson, E., Hsieh, P., Milla, K., Christensen, J., Stewart, J., Liu, X. 2008. Modeling oyster growth rate by coupling oyster population and hydrodynamic models for Apalachicola Bay, Florida, USA. Ecological Modeling 211:77-89.

Viveros, P. NOAA Graduate Research Fellowship, Phytoplankton composition and abundance in relation to salinity, nutrient and light gradients in the Apalachicola National Estuarine Research Reserve.

Anderson, C. Auburn University, School of Forestry and Wildlife Sciences. Response of coastal riverine wetlands to water allocations in an urbanizing watershed.

Smith, S. Florida A&M University post-doctoral research associate, ECSC/Environmental Sciences Institute, Drought, Reduced River Flow and Sea Level Rise: Exploring Climate Impacts on Carbon and Nitrogen Cycling in the Apalachicola Bay System.

Hagen, S., DeLorme, D., Walters, L., Wang, D., Weishampel, J., Yeh, G., Huang, W., Slinn, D., Morris, J. Ecological Effects of Sea Level Rise.

As part of the SWMP long-term monitoring program, APANERR also collects 15-minute water quality data and monthly grab and diel samples for nutrient/pigment data which may be correlated with this meteorological dataset. These data are available at [www.nerrsdata.org](http://www.nerrsdata.org).

**II. Physical Structure Descriptors**

**9) Sensor specifications –**

[Instructions/Remove: Include parameter description, units, sensor type, model #, (operating temperature), range of measurement, accuracy, (temperature dependence), (sensitivity), (stability), serial numbers, multipliers, date of last calibration, and dates in use for each sensor **(include at a minimum the sensors installed for the year covered by this metadata document)** and CR1000/CR1000X description. **Ensure that sensor information is accurate for your weather station.**]

Parameter: Temperature

Units: Celsius

Sensor type: Pt1000 Class A

Model #: EE181 Temperature and Relative Humidity Probe

Operating Temperature: -40°C to +60°C

Range: -40°C to +60°C

Accuracy: ±0.2 °C @ 23°C

S/N: 184116000295FC

Date of calibration: 05/26/2021

Dates of sensor use: 10/07/2021 - current as of 03/22/2022

S/N: 2015160012786B

Date of calibration: 04/16/2020

Dates of sensor use: 10/08/2020 – 10/07/2021

Parameter: Relative Humidity

Units: Percent

Sensor type: HC101

Model #: EE181 Temperature and Relative Humidity Probe

Range: 0-100% non-condensing

Accuracy: –15 to 40 °C: ≤90% RH ± (1.3 + 0.003 • RH reading) % RH

–15 to 40 °C: >90% RH ± 2.3% RH

–25 to 60 °C: ± (1.4 + 0.01 • RH reading) % RH

–40 to 60 °C: ± (1.5 + 0.015 • RH reading) % RH

Temperature dependence of RH measurement: typically 0.03% RH/°C

***Note:*** This sensor caps relative humidity values at 100%, measured values >100% are altered to 100%

S/N: 184116000295FC

Date of calibration: 05/26/2021

Dates of sensor use: 10/07/2021 - current as of 03/22/2022

S/N: 2015160012786B

Date of calibration: 04/16/2020

Dates of sensor use: 10/08/2020 – 10/07/2021

Parameter: Barometric Pressure

Units: millibars (mb)

Sensor type: Vaisala Barocap © silicon capacitive pressure sensor

Model #: PTB110

Operating Range: Pressure: 600 to 1060 mb; Temperature: -40°C to +60°C;

Humidity: non-condensing

Accuracy: ± 0.5 mb @ 20°C; +/- 2 mb @ 0°C to 40°C; +/- 4 mb @ -20°C to 45°C; +/- 6 mb @ -40°C to 60°C

Stability: ± 0.1 mb per year

S/N: K0220004

Date of calibration: 08/26/2019

Dates of sensor use: 08/06/2021 – current as of 03/22/2022

S/N: N4130442

Date of calibration: 12/06/2018

Dates of sensor use: 08/09/2019 – 08/06/2021

Parameter: Wind speed

Units: meter per second (m/s)

Sensor type: 18 cm diameter 4-blade helicoids propeller molded of polypropylene

Model #: R.M. Young 05103 Wind Monitor

Range: 0-60 m/s (134 mph); gust survival 100 m/s (220 mph)

Accuracy: +/- 0.3 m/s

S/N: WM131274

Date of calibration: 01/31/2017

Dates of sensor use: 04/04/2017– 01/01/2019

S/N: WM127200

Date of calibration: 03/03/2016

Dates of sensor use: 04/11/2016– 04/04/2017

S/N: 82852

Date of calibration: 08/02/2018

Dates of sensor use: 08/09/2019 – 08/06/2021

S/N: WM168479

Date of calibration: 04/16/2019

Dates of sensor use: 08/06/2021 – current as of 03/22/2022

Parameter: Wind direction

Units: degrees

Sensor type: balanced vane, 38 cm turning radius

Model #: R.M. Young 05103 Wind Monitor

Range: 360° mechanical, 355° electrical (5° open)

Accuracy: +/- 3 degrees

S/N: WM131274

Date of calibration: 01/31/2017

Dates of sensor use: 04/04/2017– 01/01/2019

S/N: WM127200

Date of calibration: 03/03/2016

Dates of sensor use: 04/11/2016– 04/04/2017

S/N: 82852

Date of calibration: 08/02/2019

Dates of sensor use: 08/09/2019 – 08/06/2021

S/N: WM168479

Date of calibration: 04/16/2019

Dates of sensor use: 08/06/2021 – current as of 03/22/2022

\*\*Note\*\* The arm of the wind sensor is checked monthly to ensure that it remains aligned to true north.

Parameter: Photosynthetically Active Radiation

Units: millimoles m-2 (total flux)

Sensor type: Un-amplified quantum sensor

Model #: SQ-110 Apogee

Light spectrum waveband: 410 to 655 nm

Temperature dependence: 0.06 ± 0.06% per °C

Stability: <±2% change over 1 yr

Operating Temperature: -40°C to 70°C; Humidity: 0 to 100%

Sensitivity: 0.2 mV per µmole m-2 s-1

Multiplier: 0.025

Field of view: 180°

S/N: 22808

Date of calibration: 05/25/2017

Dates of sensor use: 05/25/2017 – 09/30/2019

S/N: 31574

Date of calibration: 09/04/2020

Dates of sensor use: 12/08/2020 – current as of 03/22/2022

Parameter: Precipitation

Units: millimeters

Sensor type: Tipping Bucket Rain Gauge

Model #: TR525 USW

Funnel diameter: 8.0 inches

Rainfall per tip: 0.01 inch

Operating range: Temperature: 0° to 50°C; Humidity: 0 to 100%

Accuracy: +/- 1.0% up to 1 in./hr; +0, -3% from 1 to 2 in./hr; +0, -5% from 2 to 3 in./hr

S/N: 59238-314

Date of calibration: 03/08/2017

Dates sensor use: 05/14/2014 – 05/04/2018

S/N: 78181-1118

Date of calibration: 09/17/2021, previous calibration 08/08/2019

Dates of sensor use: 08/09/2019 – 09/17/2021, 09/17/2021 – current as of 03/22/2022

Units: millimeters

Sensor type: Tipping Bucket Rain Gauge

Model #: TR525 USW

Funnel diameter: 6.0 inches

Rainfall per tip: 0.01 inch

Operating range: Temperature: 0° to 50°C; Humidity: 0 to 100%

Accuracy: +/- 1.0% up to 1 in./hr; +0, -3% from 1 to 2 in./hr; +0, -5% from 2 to 3 in./hr

S/N: 74048

Date of calibration: 05/04/2018

Dates sensor use: 05/04/2018 – 01/01/2019

CR1000X

The CR1000X has 4 MB of battery backed SRAM that is used for CPU usage and Final Storage. An additional 4 MB of SRAM is used for program storage, configuration settings, and operating system storage. Another 72 MB of Flash memory is used for data storage. Additional storage is available by using a microSD (up to 16GB) flash card using the integrated reader.

CR1000X

S/N: 3360

Calibrated: 05/11/2018, calibrated/serviced 12/04/2018 after Hurricane Michael

Installed: 06/22/2018 – 10/22/2018; 08/09/2019 – current as of 12/31/2021

Removed: In use as of 12/31/2021

**CR1000/CR1000X Firmware Version (s):**

CR1000 Firmware Version 24 in use from 08:45 10/12/2012 – 14:15 02/14/2014

CR1000 Firmware Version 27 in use from 14:30 02/14/2014 – 07:30 05/04/2018

CR1000 Firmware Version 32.02 in use from 08:00 05/04/2018 - 08:00 06/22/2018

CR1000X Firmware Version 1.02 in use from 08:00 06/22/2018 –15:45 10/22/2018

CR1000X Firmware Version 2.00 in use from 10:45 08/09/2019 – 13:15 10/25/2021

CR1000X Firmware Version 5.01 in use from 14:00 10/25/2021 – current as of 12/31/2021

**CR1000/CR1000X Program Version(s):**

apaebmet\_CR1000\_5.6\_072513.CR1 in use 9:15 07/26/2013 – 12:00 01/23/2014

apaebmet\_CR1000\_5.6\_122013.CR1 in use 12:15 01/23/2014 – 10:15 01/14/2015

apaebmet\_CR1000\_5.6\_010715.CR1 in use 10:30 01/14/2015 – 10:00 02/16/2016

apaebmet\_CR1000\_5.6\_020816.CR1 in use 10:15 02/16/2016 – 10:00 04/11/2016

apaebmet\_CR1000\_5.6\_032316.CR1 in use 10:30 04/11/2016 – 08:00 06/22/2018

apaebmet\_CR1000X\_5.6\_061518.CR1X in use 08:30 06/22/2018 – 09:30 10/20/2019

apaebmet\_CR1000X\_6.0.1\_080919.CR1X in use 09:45 10/20/2019 – 10:45 02/03/2022

apaebmet\_CR1000X\_6.0.3\_012622.CR1X in use 12:45 02/03/2022 – 15:00 02/04/2022

apaebmet\_CR1000X\_6.0.3\_020422.CR1X in use 15:15 02/04/2022- current as of 12/31/2021

Transmitter: TX-325

Model: Omnisat-3

Serial Number: 300002085

Date Installed: 02/03/2022

**10) Coded variable definitions -**

Sampling station: Sampling site code: Station code:

East Bay EB apaebmet

**11) QAQC flag definitions –**

QAQC flags provide documentation of the data and are applied to individual data points by insertion into the parameter’s associated flag column (header preceded by an F\_). During primary automated QAQC (performed by the CDMO), -5, -4, and -2 flags are applied automatically to indicate data that is above or below sensor range, or missing. All remaining data are then flagged 0, as passing initial QAQC checks. During secondary and tertiary QAQC 1, -3, and 5 flags may be used to note data as suspect, rejected due to QAQC, or corrected.

-5 Outside High Sensor Range

-4 Outside Low Sensor Range

-3 Data Rejected due to QAQC

-2 Missing Data

-1 Optional SWMP supported Parameter

0 Passed Initial QAQC Checks

1 Suspect Data

2 *Open - reserved for later flag*

3 *Open - reserved for later flag*

4 Historical Data: Pre-Auto QAQC

5 Corrected Data

**12) QAQC code definitions** –

QAQC codes are used in conjunction with QAQC flags to provide further documentation of the data and are also applied by insertion into the associated flag column. There are three (3) different code categories, general, sensor, and comment. General errors document general problems with the CR1000/CR1000X, sensor errors are sensor specific, and comment codes are used to further document conditions or a problem with the data. Only one general or sensor error and one comment code can be applied to a particular data point, but some comment codes (marked with an \* below) can be applied to the entire record in the F\_Record column.

General Errors

GIM Instrument malfunction

GIT Instrument recording error, recovered telemetry data

GMC No instrument deployed due to maintenance/calibration

GMT Instrument maintenance

GPD Power down

GPF Power failure / low battery

GPR Program reload

GQR Data rejected due to QA/QC checks

GSM See metadata

Sensor Errors

SDG Suspect due to sensor diagnostics

SIC Incorrect calibration constant, multiplier or offset

SIW Incorrect wiring

SMT Sensor maintenance

SNV Negative value

SOC Out of calibration

SQR Data rejected due to QAQC checks

SSD Sensor drift

SSN Not a number / unknown value

SSM Sensor malfunction

SSR Sensor removed

Comments

CAF Acceptable calibration/accuracy error of sensor

CCU Cause unknown

CDF Data appear to fit conditions

CML Snow melt from previous snowfall event

CRE\* Significant rain event

CSM\* See metadata

CVT\* Possible vandalism/tampering

CWE\* Significant weather event

**13) Other remarks/notes** –

Data are missing due to equipment or associated specific sensors not being deployed, equipment failure, time of maintenance or calibration of equipment, or repair/replacement of a sampling station platform. Any NANs in the dataset stand for “not a number” and are the result of low power, disconnected wires, or out of range readings. If additional information on missing data is needed, contact the Research Coordinator at the reserve submitting the data.

Relative Humidity data greater than 100 are within range of the sensor accuracy of +/-3% and are flagged and coded as suspect, <1> (CAF). Values greater than 103 are rejected <-3>.

Data recorded for all parameters (with the exception of cumulative precipitation) at the midnight timestamp (00:00) are the 15 minute averages and totals for the 23:45-23:59 time period of the previous day. Cumulative precipitation data at the midnight timestamp (00:00) are the sum of raw (unrounded) precipitation data from 00:00 to 23:59 of the previous day. Summing each individual 15-minute total precipitation value from the same period will result in small differences from cumulative precipitation due to rounding. It is especially important to note how data at the midnight timestamp are recorded when using January 1st and December 31st data. **Note: Cumulative precipitation is no longer available via export from the CDMO. Please contact the reserve or the CDMO for more information or to obtain these data.**

01/02/2021 01:30 – 01/03/2021 00:00 Significant rain event, total precipitation coded for duration of event and cumulative precipitation coded through the end of the day.

03/10/2021 00:00 – 03/11/2021 23:45 FWC burning North of station, {CSM}

04/01/2021 10:45 Reject rain gauge reading was cleaning pollen buildup, cumulative precipitation rejected through the end of the day.

05/10/2021 07:30 Reject rain gauge reading was cleaning pollen buildup (CumPrcp off as result),

cumulative precipitation rejected through the end of the day.

06/21/2021 11:00 – 06/22/2021 00:00 Significant rain event, total precipitation coded for duration of event and cumulative precipitation coded through the end of the day.

07/09/2021 15:30 - 07/10/2021 00:00 Significant rain event from Tropical Storm Elsa, 07/07/2021 landfall Taylor County FL, <0> [GSM](CRE) for total; cumulative precipitation coded through the end of the day

08/06/2021 07:30 – 07:45 Reject BP, WSpd, Wdir data, replaced BP sensor and checked RM Young sensor’s directional readings

08/16/2021 00:00 – 08/17/2021 00:00 Significant weather event, Hurricane Ida, {CWE} {CSM}

09/15/2021 11:00 – 09/16/2021 00:00 Significant rain event, total precipitation coded for duration of event and cumulative precipitation coded through the end of the day.

09/16/2021 07:15 – 09/17/2021 08:45 Reject total and cumulative precipitation for rain gauge calibration. Cumulative rejections continued through the end of the day until 09/18/2021 00:00. Campbell Scientific had to be contacted for guidance.

09/30/2021 09:45 – 11/02/2021 15:15 Intermittent data drop out and Temp RH sensor issues believed to be caused by TX321 failure possibly due to nearby lightning strike, issues resolved when TX321 was finally disconnected. Missing data during this time frame are coded for instrument malfunction, <-2> [GIM](CSM). The record immediately following the gaps in data are rejected for more than likely not being a full 15 minutes of 5-second data, <-3> [GIM](CSM)

10/10/2021 2:30 – 10/13/2021 11:00; 10/14/2021 23:15 – 10/18/2021 15:45; 10/19/2021 08:00 – 10/19/2021 14:15; 10/20/2021 7:45 – 12:15, 12:45 – 14:15, 14:45 – 15:45; 10/21/2021 08:45 – 17:45; 10/22/2021 08:00 – 08:15, 08:45 – 09:30, 10:15 – 17:45; 10/23/2021 08:15 – 13:30, 14:00 – 15:30, 16:00 – 17:30; 10/25/2021; 10/26/2021 08:00 – 08:15 Reject Temp RH data, erroneous temperature readings

10/13/2021 11:15 Reject all data, station powered down

10/18/2021 14:30 Replaced logger battery, reject all data

10/20/2021 07:45 – 10/23/2021 17:30 PAR data that are not missing or rejected are considered suspect. Values were lower than expected with unknown cause but may be related to TX321 issues.

10/25/2021 13:30 Updated CR1000X OS and reloaded program file, all parameters rejected at 13:45

10/25/2021 13:45; 10/26/2021 13:10 – 13:15; 11/02/2021 15:15 Testing EE181 current, Reject Temp, RH, BP data