**Reserve Name** JOB **NERR NERR Water Quality Metadata**

**Months and year the documentation covers: 01/01/2014 to 12/31/2014**

**Latest Update: 0/28**/2016

**I. Data Set and Research Descriptors**

**1) Principal investigator(s) and contact persons**

**Jobos Bay National Estuarine Research Reserve**

**PO Box 159**

**Salinas, PR 00704-0159**

**Ph. 787-853-4617**

**Fx. 787-853-4618**

**Angel Dieppa, Research Coordinator**

**Ph. 787-853-4617**

**Email.** [**adieppa@gmail.com**](mailto:adieppa@gmail.com)**,** [**adieppa@drna.gobierno.pr**](mailto:adieppa@drna.gobierno.pr)

**Enid Malavé, Chemist, SWMP Technician**

**Ph. 787-853-4617**

**Email.** [**emalave1@gmail.com**](mailto:emalave1@gmail.com)**,** [**emalave@drna.gobierno.pr**](file:///\\drnasrv1\Investigation\Lab-pc1%20Documents\YSI2014\YSI2014\Meta%20Data%202014\emalave@drna.gobierno.pr)

**2) Entry verification**

Deployment data are uploaded from the YSI data logger to a Personal Computer (IBM compatible) by Enid Malavé. Files are exported from EcoWatch in a comma-delimited format (.CDF) and uploaded to the CDMO by Enid Malavé and Angel Dieppa where they undergo automated primary QAQC and become part of the CDMO’s online provisional database. Excessive pre- and post-deployment data are removed from the file prior to upload with up to 2 hours of pre- and post-deployment data retained to assist in data management. During primary QAQC, data are flagged if they are missing or out of sensor range. The edited file is then returned to the Reserve where it is opened in Microsoft Excel and processed using the CDMO’s NERRQAQC Excel macro by Enid Malavé and Angel Dieppa. The macro inserts station codes, creates metadata worksheets for flagged data and summary statistics, and graphs the data for review. It allows the user to apply QAQC flags and codes to the data, remove any overlapping deployment data, append files, and export the resulting data file for upload to the CDMO. Upload after secondary QAQC results in ingestion into the database as provisional plus data, recalculation of cDepth or cLevel parameters, and finally tertiary QAQC by the CDMO and assimilation into the CDMO’s authoritative online database. Where deployment overlap occurs between files, the data produced by the newly calibrated sonde is generally accepted as being the most accurate. The final yearly file and metadata was submitted by Enid Malavé and Angel Dieppa. For more information on QAQC flags and codes, see Sections 11 and 12.

**3) Research objectives**

The principal objective is to record and track long-term changes and short term variability in water quality parameters that can be associated to changes in estuarine habitats. Through this, we support management decisions based on scientific data. A secondary objective is to promote the access and use of reliable baseline information by federal and local agencies, universities, researchers, educators and local communities to enhance the process by which they make decisions regarding their daily activities. This data is also invaluable in the identification and development of future monitoring and research activities.

A total of four data loggers (YSI 6600 V2, YSI 6600 V4) are deployed in Jobos Bay. Two sondes are deployed in the inner lagoons of the Mar Negro Component and the other two in the Jobos Bay. The instruments are suspended from a pole at a distance at about 0.5 meters from the surface at each selected site. Data from stations 9, 10, 19 and 20 are being submitted to the Centralized Data Management Office as part of the System-Wide Monitoring Program. Measurements are taken at fifteen-minute intervals for approximately two-week periods. The sites are identified as representative of areas within the reserve and comparable to the sites that may be receiving impact from human activities from surroundings areas or may act as a habitat gradient in the Bay.

Station number nine (9), the impacted site, collects water quality data in a site associated with runoff from littoral and basin mangrove areas. This sampling station is located in the most inland lagoon, closest to the Thermoelectric Power Plant (oil and natural gas). It is subjected to runoff, which may include potential oil spill contamination from this industrial facility. Information compiled from historical environmental documents, indicate that station nine (9) was used as a disposal site for residues of the previously operating sugar mill operation, and therefore might have high organic input into the sediments.

Station number ten (10), located in a mangrove lagoon area towards the southwestern section of Mar Negro is considered the reference or non-impacted site.

Station number (19) is located over a sea grass bed (*Thalassia testudinum*) in the inner western part of the bay just northeast of Cayo Colchones. This station is located near the thermal outfall and operating piers of the Aguirre Power Plant Complex, both activities may have significant effects on sea grass communities. This area is exposed to barge stranding, sediment re-suspension and oil spills.

Station number (20) is located on the eastern inner bay section of the Cayos Caribe cays. This station is just south of the mangrove islets associated with the Reserve's coral reefs. Water streams coming through the coral platform may help characterize water conditions of the main marine currents reaching Jobos Bay, as well as possible effects of industrial and chemical activities associated with Phillips Core, AES Coal Energy Plant and Pharmaceuticals located just east to this system.

**4) Research methods**

The National Estuarine Research Reserve Water Quality Monitoring Program began sampling at Station nine (9) on December 20, 1995 and Station ten (10) on February 1, 1996. Monitoring at station 19 began in April 2004 and at station 20 in June 2004. Long term water quality monitoring is being performed at these stations.

Before each YSI 6600 data logger is deployed, calibration and maintenance is performed following the Standard Operation Procedures of the NEERS. Calibration standards are only required for pH, salinity, and turbidity, all other parameters are done as described in the manual. Buffer solutions for two-point calibration (pH 7 and pH 10) are purchased from a scientific supply company. Salinity is calibrated with a specific conductance standard 50 mS/cm and is purchased from YSI or a scientific supply company.

The two-point turbidity calibration is performed using a 0 NTU (DI water) and 126 NTU standard purchased from a scientific company. YSI sonde 6600 v2 and v4 are equiped with dissolved oxygen optical sensors, both are allowed to sit at least 24 hours after proper calibration. Weather conditions and tide stage are recorded in the field observation log during deployment. Measurements of DO, pH, salinity, specific conductance, turbidity, and temperature are taken at the deployment time to check the accuracy and functionality of the instruments.

Each YSI data logger is tied with steel cable to an iron galvanized pole, which is plunged into the sediments at each sampling area. Data loggers are suspended from a pole at approximately 0.5 meter from the surface of the selected site. Data is recorded every 15 minutes. The following measurements are recorded: date, time, temperature, specific conductance, salinity, dissolved oxygen saturation, dissolved oxygen concentration, depth, pH, and turbidity, all station have an optical chlorophyll-a sensor. Chl-a is an optional parameter non-required for SWMP program. Approximately, every two weeks the data loggers are retrieved, inspected, cleaned, data is dowloaded into a personal computer and re-calibrated as noted previously. The data logger is then ready to be deployed again.

The data is processed through a standard quality control/quality assurance established for all 27 reserves within the system. It consists in submitting the raw data to the Centralized Data Management Office (CDMO) server where data undergoes through a macro to flag anomalies predetermine for each station. The data is sent back to the reserve to pass through a secondary QA/QC and finally resubmitted to CDMO for the final approval. Data may be available in different stages of the QA/QC process.

A Sutron Sat-Link2 transmitter was installed at the JOB20 station on 07/20/06 and transmits data to the NOAA GOES satellite, NESDIS ID # 3B0297EC. The transmissions are scheduled hourly and contain four (4) data sets reflecting fifteen minute data sampling intervals. Upon receipt by the CDMO, the data undergoes the same automated primary QAQC process detailed in Section 2 above. The “real-time” telemetry data become part of the provisional dataset until undergoing secondary and tertiary QAQC and assimilation in the CDMO’s authoritative online database. Provisional and authoritative data are available at [http://cdmo.baruch.sc.edu](http://cdmo.baruch.sc.edu/).

**5) Site location and character –**

The Jobos Bay National Estuarine Research Reserve (JBNERR) is located on the southern coastal plain of the island of Puerto Rico, a reserve within the West Indies geographical area. JBNERR is composed of two major areas: (1) Mar Negro, located on the western margin of the Bay, and (2) Cayos Caribe (a chain of 17 tear-shaped islets located to the southeast) and Cayos Barca (a chain of 7 tear-shaped islets located to the southwest boundaries) both with a back-reef system. The Mar Negro area comprises the bulk of the Reserve, and consists of mangrove forests and a complex system of lagoons and channels interspersed with salt and mud flats. Coral reefs and sea grass beds, with small beach deposits and upland areas fringe Cayos Caribe and Cayos Barca mangrove islands. Few areas in the watershed drain directly to the bay. Rio Seco to the north-east of the bay is active only during heavy rain events during the wet season. A small creek, Quebrada Coqui, near JBNERR’s pier to the north of the bay, drains into an extensive mangrove fringe forest in a laminar flow. During heavy rain events, Station 09 received runoff water from upland and finally, a diffuse flow of water reach the bay from the local aquifer.

Station 9 is an impacted site and is located on the northeastern section of the Mar Negro component. This sampling station is associated with mangrove lagoon areas and receives runoff from mudflats, the Thermoelectric Power Plant, and adjacent areas. The tidal range varies from 12 to 14 inches near the monitoring station. The salinity at the vicinity of the monitoring station varies from 26.0 ppt to 41.1 ppt. The average depth at station 09 is 1 meter. The bottom is covered by a thick layer of thin sediments with a high content of organic material. *Microcoleous* sp. (blue-green algae), brown and green algae (*Caulerpa* sp.) are also present at this site, but a better assessment is needed. The station pole was located at 17° 56' 36.8" N and 66° 14' 18.5" W until 09/02/2010 12:00PM, then it was relocated to 17° 56' 35.0" N and 66° 14' 18.9" W approximately 65.0 meters from original position. The most up to date location for this station as of 2016 is 17° 56' 34.88"N, 66° 14' 18.64"W. The relocalization was due to sedimentation issues and the construction of a new telemetry station. Fresh water input to the station comes only from runoff and rain. This station has been subject of several studies indicating the presence of relatively high level of cooper and pesticides compared to other stations.

Station 10 is located in a mangrove lagoon not impacted directly by any upland or marine activities. It provides a reference for comparison of data obtained in other stations, especially to the station in Mar Negro lagoon. The tidal range varies from 12 to 14 inches. The salinity at the vicinity of the monitoring station varies from 27.0 ppt to 41.7 ppt. The average depth at station 10 is 1 meter. The bottom is covered with a layer of fine sediments with organic material, followed by a layer of calcareous material mainly from shells and oysters. At this site, we can find sea grass (*Thalassia*), calcareous algae (*Halimeda* sp.), green algae (*Caulerpa* sp.) and brown algae (*Dictyota* sp.) among others. The pole is located at 17° 56' 19.00"N, 66° 15' 27.85"W . Fresh water input to the station comes only from runoff and rain. There is not any direct source of fresh water.

Station 19 is located on the western inner section of the bay at a distance of 233 meters from Cayo Colchones Mangroves over sea grass beds (*Thallasia testudinum*). Tidal ranges in this area vary from 12 to 14 inches. The salinity at the vicinity of the monitoring station varies from 30.0 ppt to 36.0 ppt. The average depth at this station is of 2 meters. The YSI' sonde is deployed at about 1 foot from the bottom. The bottom is of sandy composition. Sea grass, algae, echinoderms and other related organisms could be found in the area. The pole is located at 17° 56' 34.49"N, 66° 13' 43.77"W. There is no freshwater input to this area.

Station 20 is located in the inner eastern section at about 190 meters of Cayos Caribe Mangrove islets and at about 688 meters from the coral reef barrier. This station is the closest to Mar Caribe. It has a sandy bottom, with calcareous and coral fragments, sea grass (*Thalassia*) communities, echinoderms and other associated organisms. Tidal ranges in this area vary from 12 to 14 inches. The salinity at the vicinity of the monitoring station varies from 30.0 ppt to 36.0 ppt. The average depth of the site is 2 meters. There is no freshwater input to this area. The pole is located at 17° 55' 49.14"N, 66° 12' 41.30"W.

Data from stations 9, 10, 19 and 20 is being submitted to the CDMO. Eight sondes are permanently devoted to taking readings from these two sites, to assure continuous readings while sondes are taken out of the water for data upload and maintenance. This will avoid data gaps for the stations between sonde maintenance procedures. Due to errors in calibration, turbidity data in these files is considered inadequate. All monitoring is considered long term.

**6) Data collection period –**

Station nine (9) water quality monitoring began on December 20, 1995.

Station ten (10) water quality monitoring began on February 1, 1996.

Station nineteen (19) water quality monitoring began on April 1, 2004.

Station twenty (20) water quality monitoring began on May 13, 2004.

Deployment and Retrieval Dates 2014:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |  |  |
| **Station 09** |  |  |  |  | **Station 19** |  |  |  |
| **Date/Time In** |  | **Date/Time Out** | |  | **Date/Time In** | | **Date/Time Out** | |
| 12/17/2013 | 10:00 | 01/17/2014 | 9:15 |  | 12/19/2013 | 11:30 | 1/15/2014 | 10:15 |
| 01/17/2014 | 9:45 | 1/28/2014 | 10:00 |  | 1/15/2014 | 10:45 | 1/28/2014 | 9:45 |
| 01/28/2014 | 10:30 | 02/11/2014 | 09:45 |  | 01/28/2014 | 10:00 | 02/11/2014 | 09:15 |
| 02/11/2014 | 10:00 | 02/25/2014 | 10:45 |  | 02/11/2014 | 09:45 | 02/25/2014 | 10:15 |
| 02/25/2014 | 11:00 | 03/11/2014 | 12:30 |  | 02/25/2014 | 10:30 | 03/11/2014 | 14:00 |
| 03/11/2014 | 12:45 | 03/25/2014 | 9:30 |  | 03/11/2014 | 14:15 | 03/25/2014 | 9:00 |
| 03/25/201 | 10:00 | 04/08/2014 | 10:15 |  | 03/25/201 | 9:15 | 04/08/2014 | 9:45 |
| 04/08/2014 | 10:30 | 04/23/2014 | 9:45 |  | 04/08/2014 | 10:15 | 04/23/2014 | 8:45 |
| 04/23/2014 | 10:15 | 05/06/2014 | 10:15 |  | 04/23/2014 | 9:00 | 05/06/2014 | 9:30 |
| 05/06/2014 | 10:30 | 05/20/2014 | 10:15 |  | 05/06/2014 | 9:45 | 05/20/2014 | 12:15 |
| 05/20/2014 | 10:45 | 06/03/2014 | 10:15 |  | 05/20/2014 | 12:30 | 06/03/2014 | 09:45 |
| 06/03/2014 | 10:30 | 06/16/2014 | 9:30 |  | 06/03/2014 | 10:15 | 06/16/2014 | 10:15 |
| 06/16/2014 | 10:00 | 07/01/2014 | 11:00 |  | 06/16/2014 | 10:30 | 07/01/2014 | 10:15 |
| 07/01/2014 | 11:15 | 07/15/2014 | 09:45 |  | 07/01/2014 | 10:45 | 07/15/2014 | 09:30 |
| 07/15/2014 | 10:00 | 07/31/2014 | 09:30 |  | 07/15/2014 | 09:45 | 07/31/2014 | 09:00 |
| 07/31/2014 | 09:45 | 08/12/2014 | 10:15 |  | 07/31/2014 | 09:15 | 08/12/2014 | 12:15 |
| 08/12/2014 | 10:45 | 08/26/2014 | 10:00 |  | 08/12/2014 | 12:30 | 08/26/2014 | 9:00 |
| 08/26/2014 | 10:15 | 09/09/2014 | 10:00 |  | 08/26/2014 | 09:30 | 09/09/2014 | 9:45 |
| 09/09/2014 | 10:15 | 09/23/2014 | 10:00 |  | 09/09/2014 | 10:00 | 09/23/2014 | 09:30 |
| 09/23/2014 | 10:15 | 10/07/2014 | 11:00 |  | 09/23/2014 | 09:45 | 10/07/2014 | 12:45 |
| 10/07/2014 | 11:30 | 10/22/2014 | 10:45 |  | 10/07/2014 | 13:00 | 10/22/2014 | 10:15 |
| 10/22/2014 | 11:15 | 11/4/2014 | 10:45 |  | 10/22/2014 | 10:30 | 11/4/2014 | 10:15 |
| 11/4/2014 | 11:15 | 11/18/2014 | 10:00 |  | 11/4/2014 | 10:45 | 11/18/2014 | 09:30 |
| 11/18/2014 | 10:15 | 12/02/2014 | 10:45 |  | 11/18/2014 | 09:45 | 12/02/2014 | 10:15 |
| 12/02/2014 | 11:15 | 12/16/2014 | 9:30 |  | 12/02/2014 | 10:30 | 12/16/2014 | 10:30 |
| 12/16/2014 | 09:45 | 01/13/2015 | 10:15 |  | 12/16/2014 | 10:45 | 01/13/2015 | 12:00 |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| **Station 10** |  |  |  |  | **Station 20** |  |  |  |
| **Date/Time In** |  | **Date/Time Out** | |  | **Date/Time In** | | **Date/Time Out** | |
| 12/17/2013 | 10:45 | 01/17/2014 | 09:45 |  | 12/19/2013 | 11:45 | 1/15/2014 | 10:00 |
| 01/17/2014 | 10:00 | 1/28/2014 | 10:30 |  | 1/15/2014 | 10:15 | 1/28/2014 | 09:15 |
| 01/28/2014 | 10:45 | 02/11/2014 | 10:00 |  | 01/28/2014 | 09:30 | 02/11/2014 | 08:45 |
| 02/11/2014 | 10:30 | 02/25/2014 | 12:00 |  | 02/11/2014 | 09:15 | 02/25/2014 | 09:30 |
| 02/25/2014 | 12:15 | 03/11/2014 | 13:15 |  | 02/25/2014 | 09:45 | 03/11/2014 | 11:15 |
| 03/11/2014 | 13:45 | 03/25/2014 | 09:15 |  | 03/11/2014 | 11:45 | 03/25/2014 | 08:45 |
| 03/25/201 | 9:30 | 04/08/2014 | 11:00 |  | 03/25/201 | 9:00 | 04/08/2014 | 09:15 |
| 04/08/2014 | 11:15 | 04/23/2014 | 10:45 |  | 04/08/2014 | 9:45 | 04/23/2014 | 09:15 |
| 04/23/2014 | 11:00 | 05/06/2014 | 11:00 |  | 04/23/2014 | 9:30 | 05/06/2014 | 13:30 |
| 05/06/2014 | 11:15 | 05/20/2014 | 11:15 |  | 05/06/2014 | 14:00 | 05/20/2014 | 09:45 |
| 05/20/2014 | 11:30 | 06/03/2014 | 11:00 |  | 05/20/2014 | 10:00 | 06/03/2014 | 09:15 |
| 06/03/2014 | 11:15 | 06/16/2014 | 09:15 |  | 06/03/2014 | 9:30 | 06/16/2014 | 08:30 |
| 06/16/2014 | 9:30 | 07/01/2014 | 11:30 |  | 06/16/2014 | 8:45 | 07/01/2014 | 09:45 |
| 07/01/2014 | 11:45 | 07/15/2014 | 10:45 |  | 07/01/2014 | 10:00 | 07/15/2014 | 09:00 |
| 07/15/2014 | 11:00 | 07/31/2014 | 10:15 |  | 07/15/2014 | 09:15 | 07/31/2014 | 12:30 |
| 07/31/2014 | 10:30 | 08/12/2014 | 11:15 |  | 07/31/2014 | 13:00 | 08/12/2014 | 10:00 |
| 08/12/2014 | 11:30 | 08/26/2014 | 11:00 |  | 08/12/2014 | 10:15 | 08/26/2014 | 09:15 |
| 08/26/2014 | 11:15 | 09/09/2014 | 11:00 |  | 08/26/2014 | 09:45 | 09/09/2014 | 09:15 |
| 09/09/2014 | 11:15 | 09/23/2014 | 10:30 |  | 09/09/2014 | 09:30 | 09/23/2014 | 09:00 |
| 09/23/2014 | 10:45 | 10/07/2014 | 12:00 |  | 09/23/2014 | 09:30 | 10/07/2014 | 09:30 |
| 10/07/2014 | 12:15 | 10/22/2014 | 11:30 |  | 10/07/2014 | 10:00 | 10/22/2014 | 09:45 |
| 10/22/2014 | 12:00 | 11/4/2014 | 11:45 |  | 10/22/2014 | 10:00 | 11/4/2014 | 09:45 |
| 11/4/2014 | 12:00 | 11/18/2014 | 10:45 |  | 11/4/2014 | 10:00 | 11/18/2014 | 09:00 |
| 11/18/2014 | 11:00 | 12/02/2014 | 12:00 |  | 11/18/2014 | 09:30 | 12/02/2014 | 13:45 |
| 12/02/2014 | 12:15 | 12/16/2014 | 09:45 |  | 12/02/2014 | 14:15 | 12/16/2014 | 11:15 |
| 12/16/2014 | 10:15 | 01/13/2015 | 11:15 |  | 12/16/2014 | 11:45 | 01/13/2015 | 09:45 |

**7) Distribution**

NOAA retains the right to analyze, synthesize and publish summaries of the NERRS System-wide Monitoring Program data.  The NERRS retains the right to be fully credited for having collected and process the data.  Following academic courtesy standards, the NERR site where the data were collected should be contacted and fully acknowledged in any subsequent publications in which any part of the data are used.  The data set enclosed within this package/transmission is only as good as the quality assurance and quality control procedures outlined by the enclosed metadata reporting statement.  The user bears all responsibility for its subsequent use/misuse in any further analyses or comparisons.  The Federal government does not assume liability to the Recipient or third persons, nor will the Federal government reimburse or indemnify the Recipient for its liability due to any losses resulting in any way from the use of this data.

Requested citation format:

NOAA National Estuarine Research Reserve System (NERRS). System-wide Monitoring Program. Data accessed from the NOAA NERRS Centralized Data Management Office website: <http://www.nerrsdata.org/>; *accessed* 12 October 2012.

NERR water quality data and metadata can be obtained from the Research Coordinator at the individual NERR site (please see Principal Investigators and Contact Persons), from the Data Manager at the Centralized Data Management Office (please see personnel directory under the general information link on the CDMO home page) and online at the CDMO home page [http://cdmo.baruch.sc.edu/](http://cfcdmo.baruch.sc.edu/).  Data are available in comma delimited format.

**8) Associated researchers and projects**

The Jobos Bay NERR maintains four water quality monitoring stations as part of the System Wide Monitoring Program (SWMP) to monitor variability in the estuarine environment. Meteorological station collect continuous information that support water quality data intended to address short-term variability and long-term changes in estuarine water parameters within the bay (i.e., localized impacts of seasonal storms and hurricane events, variability due to tidal circulation, seasonal and interannual differences in rainfall, magnitude and influence of major events such hurricanes, spatial extent of oceanic and tidal forcing.

Our water quality monitoring program is a key component of SWMP. Variables measured include Temperature, Dissolved Oxygen, Turbidity, pH, Salinity and Depth in 4 permanent stations equipped with YSI datasondes. The program support a nutrient monitoring at the same stations, nitrogen, phosphorus, and chlorophyll are measured in a monthly basis. Also, a diel nutrient sampling is performed in a monthly basis.

SWMP data has been used by Caribbean Regional Association for the Caribbean Regional Integrated Coastal Ocean Observing System (CaRICOOS) who monitors Real Time data from our SWMP stations.

**II. Physical Structure Descriptors**

**9) Sensor specifications –**

**YSI 6600EDS V2/ YSI 6600EDS V4 data sonde:**

Parameter: Temperature

Units: Celsius (C)

Sensor Type: Thermistor

Model#: 6560

Range: -5 to 50 C

Accuracy: +/- 0.15

Resolution: 0.01 C

Parameter: Conductivity

Units: milli-Siemens per cm (mS/cm)

Sensor Type: 4-electrode cell with autoranging

Model#: 6560

Range: 0 to 100 mS/cm

Accuracy: +/- 0.5% of reading + 0.001 mS/cm

Resolution: 0.001 mS/cm to 0.1 mS/cm (range dependant)

Parameter: Salinity

Units: parts per thousand (ppt)

Sensor Type: Calculated from conductivity and temperature

Range: 0 to 70 ppt

Accuracy: +/- 1.0% of reading pr 0.1 ppt, whichever is greater

Resolution: 0.01 ppt

Parameter: Dissolved Oxygen % saturation

Sensor Type: Optical probe w/ mechanical cleaning

Model#: 6150 ROX

Range: 0 to 500% air saturation

Accuracy: 0-200% air saturation: +/- 1% of the reading or 1% air saturation, whichever is greater 200-500% air saturation: +/- 15% or reading

Resolution: 0.1% air saturation

Units: milligrams/Liter (mg/L)

Sensor Type: Optical probe w/ mechanical cleaning

Model#: 6150 ROX

Range: 0 to 50 mg/L

Accuracy: 0-20 mg/L: +/-0.1 mg/l or 1% of the reading, whichever is greater

20 to 50 mg/L: +/- 15% of the reading

Resolution: 0.01 mg/L

Parameter: Non-vented Level - Shallow (Depth)

Units: feet or meters (ft or m)

Sensor Type: Stainless steel strain gauge

Range: 0 to 30 ft (9.1 m)

Accuracy: +/- 0.06 ft (0.018 m)

Resolution: 0.001 ft (0.001 m)

Parameter: pH – bulb probe or EDS flat glass probe

Units: pH units

Sensor Type: Glass combination electrode

Model#: 6561 or 6561FG

Range: 0 to 14 units

Accuracy: +/- 0.2 units

Resolution: 0.01 units

Parameter: Turbidity

Units: nephelometric turbidity units (NTU)

Sensor Type: Optical, 90 degree scatter, with mechanical cleaning

Model#: 6136

Range: 0 to 1000 NTU

Accuracy: +/- 2% of reading or 0.3 NTU (whichever is greater)

Resolution: 0.1 NTU

Parameter: Chlorophyll Fluorescence

Units: micrograms/Liter

Sensor Type: Optical probe w/ mechanical cleaning

Model#: 6025

Range: 0 to 400 ug/Liter

Accuracy: Dependent on methodology

Resolution: 0.1 ug/L chl a, 0.1% FS

**Dissolved Oxygen Qualifier (Rapid Pulse / Clark type sensor):**

The reliability of dissolved oxygen (DO) data collected with the rapid pulse / Clark type sensor after 96 hours post-deployment for non-EDS (Extended Deployment System) data sondes may be problematic due to fouling which forms on the DO probe membrane during some deployments (Wenner et al. 2001). Some Reserves utilize the YSI 6600 EDS data sondes, which increase DO accuracy and longevity by reducing the environmental effects of fouling. Optical DO probes have further improved data reliability. The user is therefore advised to consult the metadata for sensor type information and to exercise caution when utilizing rapid pulse / Clark type sensor DO data beyond the initial 96-hour time period. Potential drift is not always problematic for some uses of the data, i.e. periodicity analysis. It should also be noted that the amount of fouling is very site specific and that not all data are affected. If there are concerns about fouling impacts on DO data beyond any information documented in the metadata and/or QAQC flags/codes, please contact the Research Coordinator at the specific NERR site regarding site and seasonal variation in fouling of the DO sensor.

**Depth Qualifier:**

The NERR System-Wide Monitoring Program utilizes YSI data sondes that can be equipped with either depth or water level sensors. Readings for both vented and non-vented sensors are automatically compensated for water density change due to variations in temperature and salinity; but for all non-vented depth measurements, changes in atmospheric pressure between calibrations appear as changes in water depth.  The error is equal to approximately 1.03 cm for every 1 millibar change in atmospheric pressure, and is eliminated for vented sensors because they are vented to the atmosphere throughout the deployment time interval.

Beginning in 2006, NERR SWMP standard calibration protocol calls for all non-vented depth sensors to read 0 meters at a (local) barometric pressure of 1013.25 mb (760 mm/hg).  To achieve this, each site calibrates their depth sensor with a depth offset number, which is calculated using the actual atmospheric pressure at the time of calibration and the equation provided in the SWMP calibration sheet or Digital Calibration Log.  This offset procedure standardizes each depth calibration for the entire NERR System.  If accurate atmospheric pressure data are available, non-vented sensor depth measurements at any NERR site can be corrected

In 2010, the CDMO began automatically correcting depth/level data for changes in barometric pressure as measured by the Reserve’s associated meteorological station during data ingestion. These corrected depth/level data are reported as cDepth and cLevel, and are assigned QAQC flags and codes based on QAQC protocols. Please see sections 11 and 12 for QAQC flag and code definitions.

**Salinity Units Qualifier:**

In 2013, EXO sondes were approved for SWMP use and began to be utilized by Reserves. While the 6600 series sondes report salinity in parts per thousand (ppt) units, the EXO sondes report practical salinity units (psu). These units are essentially the same and for SWMP purposes are understood to be equivalent, however psu is considered the more appropriate designation. Moving forward the NERR System will assign psu salinity units for all data regardless of sonde type.

**Turbidity Qualifier:**

In 2013, EXO sondes were approved for SWMP use and began to be utilized by Reserves. While the 6600 series sondes report turbidity in nephelometric turbidity units (NTU), the EXO sondes use formazin nephelometric units (FNU). These units are essentially the same but indicate a difference in sensor methodology, for SWMP purposes they will be considered equivalent. Moving forward, the NERR System will use FNU/NTU as the designated units for all turbidity data regardless of sonde type. If turbidity units and sensor methodology are of concern, please see the Sensor Specifications portion of the metadata.

**Chlorophyll Fluorescence Disclaimer:**

YSI chlorophyll sensors (6025 or 599102-01) are designed to serve as a proxy for chlorophyll concentrations in the field for monitoring applications and complement traditional lab extraction methods; therefore, there are accuracy limitations associated with the data that are detailed in the YSI manual including interference from other fluorescent species, differences in calibration method, and effects of cell structure, particle size, organism type, temperature, and light on sensor measurements.

**10) Coded variable definitions**

Sampling station: Sampling site code: Station code:

Station 9 ST09 job09wq

Station 10 ST10 job10wq

Station 19 ST19 job19wq

Station 20 ST20 job20wq

**11) QAQC flag definitions**

QAQC flags provide documentation of the data and are applied to individual data points by insertion into the parameter’s associated flag column (header preceded by an F\_). During primary automated QAQC (performed by the CDMO), -5, -4, and -2 flags are applied automatically to indicate data that is missing and above or below sensor range. All remaining data are then flagged 0, passing initial QAQC checks. During secondary and tertiary QAQC 1, -3, and 5 flags may be used to note data as suspect, rejected due to QAQC, or corrected.

-5 Outside High Sensor Range

-4 Outside Low Sensor Range

-3 Data Rejected due to QAQC

-2 Missing Data

-1 Optional SWMP Supported Parameter

0 Data Passed Initial QAQC Checks

1 Suspect Data

2 *Open - reserved for later flag*

3 Calculated data: non-vented depth/level sensor correction for changes in barometric pressure

4 Historical Data: Pre-Auto QAQC

5 Corrected Data

**12) QAQC code definitions**

QAQC codes are used in conjunction with QAQC flags to provide further documentation of the data and are also applied by insertion into the associated flag column. There are three (3) different code categories, general, sensor, and comment. General errors document general problems with the deployment or YSI datasonde, sensor errors are sensor specific, and comment codes are used to further document conditions or a problem with the data. Only one general or sensor error and one comment code can be applied to a particular data point, but some comment codes (marked with an \* below) can be applied to the entire record in the F\_Record column.

General Errors

GIC No instrument deployed due to ice

GIM Instrument malfunction

GIT Instrument recording error; recovered telemetry data

GMC No instrument deployed due to maintenance/calibration

GNF Deployment tube clogged / no flow

GOW Out of water event

GPF Power failure / low battery

GQR Data rejected due to QA/QC checks

GSM See metadata

Corrected Depth/Level Data Codes

GCC Calculated with data that were corrected during QA/QC

GCM Calculated value could not be determined due to missing data

GCR Calculated value could not be determined due to rejected data

GCS Calculated value suspect due to questionable data

GCU Calculated value could not be determined due to unavailable data

Sensor Errors

SBO Blocked optic

SCF Conductivity sensor failure

SDF Depth port frozen

SDG Suspect due to sensor diagnostics

SDO DO suspect

SDP DO membrane puncture

SIC Incorrect calibration / contaminated standard

SNV Negative value

SOW Sensor out of water

SPC Post calibration out of range

SQR Data rejected due to QAQC checks

SSD Sensor drift

SSM Sensor malfunction

SSR Sensor removed / not deployed

STF Catastrophic temperature sensor failure

STS Turbidity spike

SWM Wiper malfunction / loss

Comments

CAB\* Algal bloom

CAF Acceptable calibration/accuracy error of sensor

CAP Depth sensor in water, affected by atmospheric pressure

CBF Biofouling

CCU Cause unknown

CDA\* DO hypoxia (<3 mg/L)

CDB\* Disturbed bottom

CDF Data appear to fit conditions

CFK\* Fish kill

CIP \* Surface ice present at sample station

CLT\* Low tide

CMC\* In field maintenance/cleaning

CMD\* Mud in probe guard

CND New deployment begins

CRE\* Significant rain event

CSM\* See metadata

CTS Turbidity spike

CVT\* Possible vandalism/tampering

CWD\* Data collected at wrong depth

CWE\* Significant weather event

**13) Post deployment information**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **STATION 09** |  |  | **Post Deployment Calibration Values** |  |  |
| **Date In** | **Date Out** | **SpCond (50mS/cm)** | **DO%** | **pH (7)** | **Turb (0 NTU)** |
| 12/17/2013 | 1/17/2014 | 46.15 | 98.6 | 7.08 | 1.8 |
| 1/17/2014 | 1/28/2014 | 48.23 | 101.4 | 7.04 | 0 |
| 1/28/2014 | 2/11/2014 | 48.07 | 102.7 | 7.15 | 0.6 |
| 2/11/2014 | 2/25/2014 | 49.64 | 98.5 | 7.05 | 0.9 |
| 2/25/2014 | 3/11/2014 | 48.23 | 101.2 | 7.07 | 0 |
| 3/11/2014 | 3/25/2014 | 50.03 | 95.7 | 7.1 | -0.1 |
| 3/25/2014 | 4/8/2014 | 49.89 | 100.2 | 7.16 | 8.4 |
| 4/8/2014 | 4/23/2014 | 49.10 | 91.7 | 7.00 | -0.6 |
| 4/23/2014 | 5/6/2014 | 47.42 | 97.8 | 7.14 | 0.8 |
| 5/6/2014 | 5/20/2014 | 49.79 | 99.1 | 7.00 | -0.8 |
| 5/20/2014 | 6/3/2014 | 47.80 | 99.6 | 7.00 | 4.7 |
| 6/3/2014 | 6/16/2014 | 48.74 | 88.9 | 6.99 | 0.1 |
| 6/16/2014 | 7/1/2014 | 48.58 | 100 | 6.99 | 1.2 |
| 7/1/2014 | 7/15/2014 | 48.00 | 99.5 | 6.93 | 0 |
| 7/15/2014 | 7/31/2014 | 50.56 | 89.9 | 6.99 | 0 |
| 7/31/2014 | 8/12/2014 | 47.90 | 91.9 | 7.09 | 0 |
| 8/12/2014 | 8/26/2014 | 49.72 | 99.6 | 7.23 | 0 |
| 8/26/2014 | 9/9/2014 | 47.88 | 99.4 | 6.95 | 0 |
| 9/9/2014 | 9/23/2014 | 47.66 | 98.7 | 7.15 | `-0.3 |
| 9/23/2014 | 10/7/2014 | 46.77 | 99.6 | 6.95 | -0.1 |
| 10/7/2014 | 10/22/2014 | 48.93 | 94 | 7.40 | 0.4 |
| 10/22/2014 | 11/04/2014 | 47.90 | 96.8 | 7.15 | 0.0 |
| 11/04/2014 | 11/18/2014 | 49.02 | 100 | 7.04 | 0.1 |
| 11/18/2014 | 12/02/2014 | 50.20 | 97.1 | 7.12 | 2.0 |
| 12/02/2014 | 12/16/2014 | 48.61 | 99.2 | 7.06 | 0 |
| 12/16/2014 | 01/13/2015 | 48.22 | 92.5 | 7.01 | 0 |
|  |  |  |  |  |  |
| **STATION 10** |  |  | **Post Deployment Calibration Values** |  |  |
| **Date In** | **Date Out** | **SpCond (50mS/cm)** | **DO%** | **pH (7)** | **Turb (0 NTU)** |
| 12/17/2013 | 1/17/2014 | 46.89 | 98.9 | 7.18 | 314.7 |
| 1/17/2014 | 1/28/2014 | 47.34 | 99.1 | 7.14 | 0.6 |
| 1/28/2014 | 2/11/2014 | 47.85 | 99.6 | 7.11 | 1.8 |
| 2/11/2014 | 2/25/2014 | 49.49 | 94.2 | 7.02 | 0.9 |
| 2/25/2014 | 3/11/2014 | 47.75 | 95.9 | 7 | 1.4 |
| 3/11/2014 | 3/25/2014 | 49.82 | 99.5 | 7.05 | 0.7 |
| 3/25/2014 | 4/8/2014 | 49.48 | 99.9 | 7.02 | 1.9 |
| 4/8/2014 | 4/23/2014 | 48.44 | 99.7 | 7.17 | 0.1 |
| 4/23/2014 | 5/6/2014 | 49.26 | 99.8 | 6.99 | 0.1 |
| 5/6/2014 | 5/20/2014 | 50.66 | 97 | 7.02 | -0.1 |
| 5/20/2014 | 6/3/2014 | 49.56 | 98.1 | 6.99 | 0.5 |
| 6/3/2014 | 6/16/2014 | 50.35 | 98.5 | 7.00 | 0 |
| 6/16/2014 | 7/1/2014 | 49.35 | 99.5 | 7.31 | 1.5 |
| 7/1/2014 | 7/15/2014 | 48.42 | 99.8 | 7.04 | 0.1 |
| 7/15/2014 | 7/31/2014 | 50.37 | 100.3 | 6.99 | 0.2 |
| 7/31/2014 | 8/12/2014 | 49.82 | 97.1 | 7.09 | -0.7 |
| 8/12/2014 | 8/26/2014 | 51.33 | 102.7 | 7.15 | -0.1 |
| 8/26/2014 | 9/9/2014 | 48.60 | 100 | 7.00 | -0.2 |
| 9/9/2014 | 9/23/2014 | 49.21 | 99 | 7.10 | 0.5 |
| 9/23/2014 | 10/7/2014 | 49.03 | 100.2 | 6.91 | 4.2 |
| 10/7/2014 | 10/22/2014 | 47.11 | 99 | 6.95 | 0.5 |
| 10/22/2014 | 11/04/2014 | 48.91 | 97.1 | 7.02 | 0.2 |
| 11/04/2014 | 11/18/2014 | 49.17 | 102 | 7.11 | -0.9 |
| 11/18/2014 | 12/02/2014 | 50.34 | 99.3 | 7.06 | 0.4 |
| 12/02/2014 | 12/16/2014 | 49.26 | 99.4 | 6.78 | -0.7 |
| 12/16/2014 | 01/13/2015 | 49.2 | 98.3 | 7 | 0.4 |
|  |  |  |  |  |  |
| **STATION 19** |  |  | **Post Deployment Calibration Values** |  |  |
| **Date In** | **Date Out** | **SpCond (50mS/cm)** | **DO%** | **pH (7)** | **Turb (0 NTU)** |
| 12/19/2013 | 1/15/2014 | 50.27 | 100.7 | 7.05 | 1.2 |
| 1/15/2014 | 1/28/2014 | 48.62 | 100.3 | 7.10 | 0.4 |
| 1/28/2014 | 2/11/2014 | 48.6 | 99.9 | 7.13 | 1 |
| 2/11/2014 | 2/25/2014 | 49.61 | 97.1 | 7.11 | 0 |
| 2/25/2014 | 3/11/2014 | 49.13 | 98 | 7.01 | 0.4 |
| 3/11/2014 | 3/25/2014 | 50.11 | 100.1 | 7.08 | 0.1 |
| 3/25/2014 | 4/8/2014 | 48.45 | 102.1 | 7.2 | 4.3 |
| 4/8/2014 | 4/23/2014 | 48.31 | 99.8 | 7.02 | 0 |
| 4/23/2014 | 5/6/2014 | 49.06 | 98.5 | 7.12 | 2.7 |
| 5/6/2014 | 5/20/2014 | 51.31 | 100.6 | 6.94 | -0.4 |
| 5/20/2014 | 6/3/2014 | 49.17 | 98.3 | 7.00 | 0.5 |
| 6/3/2014 | 6/16/2014 | 48.70 | 100.1 | 7.09 | -0.8 |
| 6/16/2014 | 7/1/2014 | 49.12 | 100.2 | 7.11 | 0.6 |
| 7/1/2014 | 7/15/2014 | 49.57 | 100.8 | 7.00 | -0.8 |
| 7/15/2014 | 7/31/2014 | 51.46 | 100 | 7.04 | 0.1 |
| 7/31/2014 | 8/12/2014 | 49.51 | 98.1 | 7.02 | 0.0 |
| 8/12/2014 | 8/26/2014 | 50.5 | 99.5 | 7.06 | 0.6 |
| 8/26/2014 | 9/9/2014 | 49.30 | 101.4 | 7.00 | 0.2 |
| 9/9/2014 | 9/23/2014 | 48.91 | 98.7 | 7.07 | 1.5 |
| 9/23/2014 | 10/7/2014 | 48.37 | 99.3 | 7.01 | 0.5 |
| 10/7/2014 | 10/22/2014 | 48.36 | 98.7 | 6.98 | 0.2 |
| 10/22/2014 | 11/04/2014 | 50.51 | 99 | 7.01 | -0.6 |
| 11/04/2014 | 11/18/2014 | 49.35 | 100.7 | 7.08 | 0.4 |
| 11/18/2014 | 12/02/2014 | 49.31 | 98.2 | 7.03 | 0.5 |
| 12/02/2014 | 12/16/2014 | 48.57 | 99.6 | 7.03 | 0.1 |
| 12/16/2014 | 01/13/2015 | 50.1 | 99.5 | 7.14 | 2.5 |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **STATION 20** |  |  | **Post Deployment Calibration Values** |  |  |
| **Date In** | **Date Out** | **SpCond (50mS/cm)** | **DO%** | **pH (7)** | **Turb (0 NTU)** |
| 12/19/2013 | 1/15/2014 | 49.32 | 100.3 | 7.17 | 2.8 |
| 1/15/2014 | 1/28/2014 | 48.40 | 99.1 | 7.06 | 2.7 |
| 1/28/2014 | 2/11/2014 | 48.37 | 97.7 | 7.28 | 0.3 |
| 2/11/2014 | 2/25/2014 | 49.33 | 99.2 | 7.02 | 0.7 |
| 2/25/2014 | 3/11/2014 | 48.41 | 97.7 | 7.1 | 0 |
| 3/11/2014 | 3/25/2014 | 48.4 | 97.4 | 7.1 | 0 |
| 3/25/2014 | 4/8/2014 | 48.51 | 98.8 | 7.12 | 2 |
| 4/8/2014 | 4/23/2014 | 50.36 | 97.1 | 7.13 | 0 |
| 4/23/2014 | 5/6/2014 | 48.07 | 98.9 | 7.01 | 0.9 |
| 5/6/2014 | 5/20/2014 | 50.27 | 97.5 | 7.09 | 0 |
| 5/20/2014 | 6/3/2014 | 47.70 | 99.2 | 6.96 | 0.9 |
| 6/3/2014 | 6/16/2014 | 49.80 | 99.8 | 7.10 | 0.1 |
| 6/16/2014 | 7/1/2014 | 48.22 | 100.3 | 7.23 | 5.6 |
| 7/1/2014 | 7/15/2014 | 48.86 | 101.4 | 7.04 | -0.1 |
| 7/15/2014 | 7/31/2014 | 50.25 | 100.4 | 7.10 | 1.7 |
| 7/31/2014 | 8/12/2014 | 47.86 | 98.4 | 7.39\* | 18.0 |
| 8/12/2014 | 8/26/2014 | 49.8 | 105.8 | 6.97 | 1.2 |
| 8/26/2014 | 9/9/2014 | 49.15 | 100.8 | 7.06 | 170.1 |
| 9/9/2014 | 9/23/2014 | 48.04 | 100.2 | 7.07 | 0.6 |
| 9/23/2014 | 10/7/2014 | 47.76 | 99.9 | 7.06 | 52.9 |
| 10/7/2014 | 10/22/2014 | 46.80 | 96.9 | 7.13 | 0.2 |
| 10/22/2014 | 11/04/2014 | 49 | 98 | 7.16 | 0.5 |
| 11/04/2014 | 11/18/2014 | 48.32 | 95.9 | 6.45 | 0.2 |
| 11/18/2014 | 12/02/2014 | 49.95 | 98.6 | 7.07 | 1.2 |
| 12/02/2014 | 12/16/2014 | 47.4 | 98.8 | 7.05 | 0 |
| 12/16/2014 | 01/13/2015 | 48.69 | 96.9 | 7.08 | 1.5 |

**\*Bad sensor**

**14) Other remarks/notes**

Data are missing due to equipment or associated specific probes not being deployed, equipment failure, time of maintenance or calibration of equipment, or repair/replacement of a sampling station platform. Any NaNs in the dataset stand for “not a number” and are the result of low power, disconnected wires, or out of range readings. If additional information on missing data is needed, contact the Research Coordinator at the reserve submitting the data.

**Conductivity/Salinity**

**JOB09WQ** From 01/21/14 at 18:45 to 1/22/14 at 8:45 low conductivities/salinities. Cause unknown but

suspect as a groundwater discharge.

**JOB20WQ** From 3/11/14 at 11:45 to 3/25 at 8:45 Cond/Salinity values higher than previous and post

deployments.

**JOB20WQ** From 11/07/14 at 12:00 to 11/07/14 at 16:45. Significant Rain Event (CRE) low conductivities/salinities, rain event on 11/06/14 3.95 inches.

**JOB20WQ** From 12/02/14 at 14:15 to 12/16/14 at 11:15. Data collected a wrong depth due to issues with hanging cable. Data seems to fit conditions.

**JOB09WQ** From 08/26/14 at 10:15 to 08/31/14 at 19:30 and 09/09/14 at 10:15 to 9/23/14 at 10:00 low conductivities/salinities, rain event on 8/22/14 and 8/23/14.

**JOB09WQ** From 11/07/14 at 15:30 to 11/13/14 at 18:45 Significant Rain Event (CRE) low conductivities/salinities, rain event on 11/06/14 3.80 inches.

**JOB10WQ** From 8/22/14 at 15:45 to 8/26/14 at 11:00 low conductivities/salinities, rain event at 8/22/14 and 8/23/14.

**JOB10WQ** From 09/07/14 at 03:45 to 09/12/14 at 5:00 low conductivities/salinities, rain event at 9/7/14.

**JOB10WQ** From 11/07/14 at 21:45 to 11/17/14 at 8:00 Significant Rain Event (CRE) low conductivities/salinities, rain event on 11/06/14 3.95 inches.

**JOB19WQ** From 9/07/14 at 20:30 to 9/09/14 at 09:45 low conductivities/salinities, rain event at 9/6/14.

**JOB19WQ** From 11/07/14 at 08:15 to 11/12/14 at 10:00 Significant Rain Event (CRE) low conductivities/salinities, rain event on 11/06/14 3.95 inches.

**JOB09WQ** From 12/16/14 at 06:45 to 09:30 small crab in the c/t sensor that affected data.

**pH Data**

**JOB20WQ** From 1/28/14 at 9:30 to 2/11/14 at 8:45 pH values higher than average.

**JOB20WQ** From 8/1/14 at 1:30 to 8/12/14 at 10:00 pH slope post calibration out of range, sensor drift.

**JOB20WQ** From 11/04/14 at 10:00 to 11/18/14 at 9:00 pH data jumped to lower values. Suspect to sensors diagnostics at post-deployment check.

**JOB20WQ** From 12/02/14 at 14:15 to 12/16/14 at 11:15. Data collected a wrong depth due to issues with hanging cable. Data seems to fit conditions.

**Chlorophyll Data**

**JOB10WQ**: -From 1/25/14 at 16:15 to 1/28/14 at 10:30 “biofouling” algae blocking the optic eyes.

**JOB10WQ**: -From 8/20/14 at 14:16:25 to 8/26/14 at 11:00 sensor drift.

**JOB09WQ**: -From 09/17/14 at 16:45 to 9/23/14 at 10:00 sensor drift reading high values.

**JOB09WQ**: -From 10/07/14 at 11:15 to 10/22/14 at 10:45 no chl-a sensor deployed.

**JOB19WQ**: -From 10/23/14 at 00:46:22 to 11/04/14 at 10:15 sensor drift reading high values.

**JOB10WQ**: -From 11/18/14 at 11:00 to 01/13/15 at 11:15 no chl-a sensor deployed.

**JOB20WQ** From 12/02/14 at 14:15 to 12/16/14 at 11:15. Data collected a wrong depth due to issues with hanging cable. Data seems to fit conditions.

**Turbidity Data**

**JOB09WQ**: -From 1/1/14 at 0:00 to 1/17/14 at 9:15, sensor drift due to biofouling, sediment

and barnacles blocking the optics. Data drift started on 12/25/13.

**JOB09WQ**: -From 04/06/14 at 22:30 to 4/8/14 at 10:15sensor drift due to biofouling, sediment

blocking the optics

**JOB09WQ**: -From 09/09/14 to 9/23/14 sensor drift due to bad wiper parkingblocking the optics and

reading high values.

**JOB10WQ**: -From 12/17/13 (1/1/14) to 1/17/14 at 9:45, sensor drift due to biofouling, hydroids,

tunicates, algae, and barnacles blocking the optics.

**JOB10WQ**: From 3/23/14 at 18:45 to 3/25/14 at 9:15 sensor drift.

**JOB19WQ**: -From 4/13/2014 to 4/23/2014, sensor drift due to biofouling, octopus and crab inside cup

blocking the optics.

**JOB19WQ**: -From 5/7/2014 to 5/20/2014, sensor drift due to biofouling, crab inside cup

blocking the optics.

**JOB19WQ**: -From 7/3/2014 to 7/14/2014 and 7/31/14 to 8/12/2014 high values due to biofouling, crab

inside cup blocking the optics several times.

**JOB19WQ**: -From 8/12/2014 to 8/25/2014 high values due to biofouling, crab inside

cup blocking the optics several times.

**JOB19WQ**: -From 10/09/2014 to 10/22/2014 high values due to biofouling, optic sensor return without

sponge on wiper.

**JOB20WQ**: -From 7/31/14 to 8/12/2014 and 9/23/14 to 10/07/14 high values. No apparent reason, sensor

read right values at station during the pre deployment field check but after connecting it to the real time station the values jumped from -0.8 to 20 NTU consistently during the full deployment.

**JOB19WQ** From 07/15/14 at 09:45 to 07/31/14 at 09:00. Data collected a wrong depth due to issues with hanging cable. Data seems to fit conditions.

**JOB20WQ** From 12/02/14 at 14:15 to 12/16/14 at 11:15. Data collected a wrong depth due to issues with hanging cable. Data seems to fit conditions.

**Notes:**

**Sensor’s serial number in sonde’s serial number.**

**JOB10WQ**: - On 2/10/14 pH, turbidity, and chlorophyll sensors new in F0319AB

On 8/14/14 turbidity 13M101240sensor new in 07M100799.

On 8/21/14 conductivity sensor 12B100451new in 07M100799.

From 8/26/14 at 11:15 to 9/9/14 at 11:00 sonde was deployed at wrong depth (GSM). Data

seems to fit conditions, no water column stratification.

On 9/4/14 pH and turbidity sensors new in D0765AA

On 10/22/14 at 11:45 data collected at wrong depth (CWD).

On 12/16/14 at 10:00 data collected at wrong depth (CWD).

**JOB09WQ**:- On 1/27/14 pH, turbidity, ROX and chlorophyll sensors new in 02J0915AA.

On 3/6/14 pH and chlorophyll sensor new in 02A0155AA

On 3/6/14 ROX membrane replaced sensor new in F 0319AB 11E10105

On 7/15/14 Installed ISCO Sampler from 9:55 to 10:15

On 8/06/14 chlorophyll sensors 13M102023 new in 02A0155AD.

On 8/21/14 turbidity sensors 13M101239 new in02A0155AA.

On 10/01/14 conductivity sensor 13A101461new in F 0319AB.

On 10/29/14 pH sensor 14F-6561new in F 0319AB.

On 11/24/14 replaced chlorophyll sensor with 12B100159 in F0319AB.

**JOB19WQ**: - On 7/29/14 conductivity sensor new 13M100258 in 01K0080AB

On 8/21/14 turbidity sensor new 13M101239 in 01K0080AB

From 7/15/14 to 7/31/14 sonde was deployed at wrong depth (GSM). Data

seems to fit conditions, no water column stratification.

On 11/24/14 turbidity sensors 14F100913 new in 02A0155AD

**JOB20WQ**: - On 1/27/14 chlorophyll sensor new in 06B2025AB

On 8/6/14 ROX membrane replaced 12B100064 in sensor 11K101365 from 06B2025AB

On 8/14/14 pH 13M and chlorophyll sensors new in 02J0915AA.

On 8/21/14 pH 13A and conductivity 12B100451sensors new in 02J0915AA

On 9/18/14 turbidity sensor new 14F100914 sensors new in 02J0915AA

On 11/14/14 pH sensor new 14F-6561 sensors new in 02J0915AA

On 11/25/14 pH 14F-6561 sensor new in 06B2025AB.

**Other:**

**Significant rain events:**

On 4/09/14 we registered a 1.40 inches of rain.

On 5/11/14 we registered a 1.38 inches of rain.

On 8/2/2014 Bertha Storm 0.85 inches of rain.

On 8/8 2014 Tropical storm 0.58 inches of rain

On 8/9/2014 Tropical storm 0.80 inches of rain.

On 8/22/2014 Tropical storm 2.65 inches of rain.

On 8/23/2014 Tropical storm 1.03 inches of rain.

On 8/29/2014 we registered 0.75 inches of rain.

On 9/7/14 we registered a 1.55 inches of rain

On 11/6/14 we registered a 3.95 inches of rain

On 12/15/14 we registered 0.77 inches of rain